23JUL14

TOTAL OPEN AREAS

WHEN PANELS CUT FROM HOOD

**The Law of Physics, re: cooling: ”There’s no substitute for square inches!”™**

-In Descending Order, By Size of Opening Area-

MODEL/SIZE HOOD LOUVER DIMENSIONS TOTAL OPENING AREA\*

IN HOOD – PER SET,

IN SQUARE INCHES

XXL 17” x 28” (2 per Set) 780

Wide-Flow 32” x 17” (1 per Set) 450

XL 13” x 21” (2 per Set) 418

Long 7 ½” x 33” (2 per Set) 342

Short & Wide 19” x 10” (2 per Set) 280

Large 11” x 17” (2 per Set) 270

Semi-Long Straight Cut 7” x 23” (2 per Set) 210

Semi-Long Angle Cut 7” x 22 ¼” (2 per Set) 202

Medium 9” x 14” (2 per Set) 168

Side Louvers-18” 2 11/16” x 18” (2 per Set) 69

Side Louvers-12” 2 11/16” x 12.5” (2 per Set) 45

\* For actual “Flow Opening”, with Louvers in place, deduct 10% for Hi-Flow™; 25% for Regular-Flow,

(Reg.-Flow available only on Size Medium and Size Large; Hi-Flow also available on these).